[image: image1.png]18 PWDE9104_ABCD_SPACE_RUNNER_SPACE_WAGON_WM_2
Fle Edt Vew Document Toos Window Help

=lolx|

G D[eis

= K| &

23-34

[ow - = (] (e

AUTOMATIC TRANSMISSION - Service Adjustment Procedures

|T:'neck tems

Check procedures.

Check conditions

Normal value

Probable cause (or remedy) if a
malfunction is found

Vehicle speed

reed switch

o Data reading
® item No. 38

Vehicle stopped

0 km/h (0 mph)

Driving at 30 km/h (19 mph)

30 km/h (19 mph)

Driving at 50 km/h (31 mph)

50 km/h (31 mph)

® Vehicle speed reed switch
malfunction if high-speed
signals emitted while vehicle is
stopped
Otherwise, vehicle speed reed
switch or Gircuit harness
malfunction

PCSV duty
 Data reading
o item No. 45

D range; idiing

50-70%

D range; 1st gear

D range; during shift

Changes ocour
according to conditions

Duty should become 100%
when, while idiing in D range,
accelerator is pressed even
slightly

TCU malfunction

TPS Malfunction

Accelerator switch system
malfunction

Amount of
damper clutch
slip.

® Data reading
ltem No. 47

D range, 3rd gear 1,500 r/min
{reading on tachometer)

100-300 r/min.

D range, 3rd gear 3500 r/min
{reading’on tachometer)

0 r/min.

Damper clutch is defective

Ignition signal line or pulse

gonarator systom is defeciv.
ransmission hydraulic pressure
is inadequate.

Damper clutch control solenoid

valve (DCCSV) is defective.

DCCSV auty
® Data reading

® Item No. 49

D range, 3rd gear 1,500 r/min
(reading on tachometer)

0%

D range, 3rd gear 3,500 r/min.
{reading’on tachometer)

Change according to
negative load

Transmission control unit is
defective.

TPS system is defective.
Pulse generator B system is
defective.
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Starter motor won't function

Clutch slips at D (tah rpm o0 high!

Cutch sips at 7 fstall o 100 high!

Venicle moves at P or N

Parking doesn't hoid

“Ronormal viraton shock when

St DELR

x| @| €nane stats when N — 0 or &

Pl dirg o —
pertomance maluncion =
mprove ustment of martal Tnkege AR

Malfunction of toraue converior

‘Operation malfuncton of of pums

Walfurction of ono-way cutch

Damaged or worn gear ot othr oty par o mPIGBeT
it of the oo "

Mallnciion of parking mechansm

Cracked dnve plte. or oose bolt

Worn made demeter of font chich etaner
Low Tlod Jevel

Line pressuro to0 low (seal Gomaged_leakage. looseness. etc]

®|x

‘Malunction of vaie body (sicking vabe, workng cauty
adusiment, atc)

® (8|9

@ (8|9

Malunctin of front citch or pistor

x| ® [8|@|x

x| x [®|x|x

Mallnction of ear cuich or prsion

Mafunciion of ickdown band or o

Improper sdusiment of xekdown sero.

Maluncten of owreverse brake or pston

Cing of oweverse biake Cicut between vaive
bochang case ot msiled

Mafoncton of end duich o pon (check bal hale, oiher

Mafuncton of biors swich. demaged or
Ssconmecied wiieg. o improper adustment o

Matuncion of TPS_or meroper adjusiment

Puise generetor (A) damaged of disconeciad
wirng o horcreut

2

Pulse generstor (B) damaged of dsconnected
wiring o1 horcrcut

Malfuncton of kickdown serve swich

I

SCSVA or B demaged or dscomnecied wing,
or shortSicuit o socking (vae pen

2

Mafuncton of gniven signal system

%

Incorrecty grounded ground susp

PCSV damaged or disconnected wirng. or shortarcut

PCSV camaged or disconnoctad wirng ialve apenl

Electonic conra system

il

'DCCSV damages or dsconnecting warng vave ciosed)

%

DCCSV shortcreut or sucking haive open]

Mauncion of overdive contrl swrich

‘Maluncton of sccolerator swich, or improper sdusiment

Maluncion of aitemporature sensor

s l52]s

Malunction of lead swich

Poor conact of ignton swich

Malunction of nsmission contal Ut

NOTE: ® indicates items of high priority during inspection.





